**How to make your Q Station works better**


**Why use Ethernet cable instead of Wi-Fi connection?**

Because Ethernet connection is a physical connection which is more stable than Wi-Fi connection. Customers can get better experience while using our product. That's why we recommend you use Ethernet cable instead of Wi-Fi connection.

**Step 1. Connect LAN cable to your home router and audio cable to your audio system**

a. Plug Ethernet cable one end to you regular router (use one of the LAN ports in the back) and the other end to Ethernet port of Q Station

b. Plug audio cable from audio out of your Q Station to your audio system.



**Step 2. Encrypt your Wi-Fi connection**

By default, Q Station SSID is “bellnetXXXXXX”. No Encryption.


(XXXXXX is the last 6 digit of your MAC)

For security reason, we recommend you'd better add password to your Wi-Fi connection.


a. Use your computer or smart phone to connect the Wi-Fi connection of your Q Station.

b. Access 172.16.0.1 via IE or any other Internet browser.


c. Click “Basic Settings”, to enter the management page



d. Change the SSID and select Wi-Fi encryption, then type the password and confirm it.



When you complete all above steps, now all things you need to do is wait about 20 seconds for Wi-Fi restarting.



**Step 3. Light control**

a. Connect your iPhone or any other smart phone to your home Wi-Fi connection

b. Play music, then switch Speaker to your Q Station.

Now you can enjoy your music lightshows.

